{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Munka1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Munka1","index":0,"n_rows":56,"n_cols":5,"rows_kept":56,"cut":false,"hidden":false,"merged":[[55,0,55,4],[1,2,1,4],[2,2,2,4],[3,0,3,4],[53,0,53,4],[54,0,54,4]],"flags":["formulas_cached_only"]}
[]
[null,null,"Fóliázott 3D bútorfrontok"]
[null,null,"minimum tele ajtó méretei 2023.02.20-tól"]
[]
["Kód","Minta","Minimum magasság (mm)","Minimum szélesség (mm)","Él profil"]
["M011","BELLO",230,200,"Bello"]
["M012","BELLO CLASSIC",293,285,"Cédrus"]
["M021","SERIE",250,265,"Bello"]
["M041","SUPERBO-A",200,200,"Bello"]
["M042","SUPERBO-B",230,230,"Bello"]
["M043","SUPERBO A EASY",200,200,"R3"]
["M051","SAPONE",115,295,"Sapone"]
["M053","SAPONE-U",115,295,"Sapone-U"]
["M081","FIUME",115,295,"Sapone"]
["M130","SVÉD-ORLO (ÚJ)",245,245,"R3"]
["M132","ORLO II",245,245,"Bello"]
["M133","RETRO-A",590,295,"Bello"]
["M134","RETRO-B",590,295,"Bello"]
["M141","TENDA",230,230,"Bello"]
["M191","MANIGLIA-L",125,295,"R3"]
["M192","MANIGLIA-U",115,100,"R3"]
["M193","MANIGLIA-S",125,295,"R3"]
["M194","MANIGLIA-C",125,295,"R3"]
["M221","INTARSIO TÖLGY",495,295,"R3"]
["M222","INTARSIO DIÓ",495,295,"R3"]
["M281","CUBICO TÖLGY",210,210,"R3"]
["M282","CUBICO DIÓ",210,210,"R3"]
["M291","DECOWOOD TÖLGY",125,295,"45°"]
["M292","DECOWOOD DIÓ",125,295,"45°"]
["M331","DECOMANIGLIA TÖLGY",125,295,"45°"]
["M332","DECOMANIGLIA DIÓ",125,295,"45°"]
["M341","ITALI",230,230,"Bello"]
["M342","ITALI CLASSIC",293,275,"Cédrus"]
["M351","LÁMPA PANEL",100,100,"Választható"]
["M410","TOWER STEP (ÚJ)",195,195,"45°"]
["M413","TOWER EASY",150,150,"R3"]
["M415","TOWER MODERN-A",195,195,"R3"]
["M416","TOWER MODERN-B",195,195,"R3"]
["M419","TOWER SLIM (ÚJ)",175,175,"R3"]
["M420","TOWER SAM (ÚJ)",265,265,"SAM"]
["M421","ISEUM",275,275,"Cédrus"]
["M431","VIOLA",200,200,"Bello"]
["M441","FUTURO","-","-","D20"]
["M501","FORTUNA",230,245,"Bello"]
["M502","FORTUNA CLASSIC",293,275,"Cédrus"]
["M541","BRANDO",195,195,"R8"]
["M642","LIA-MODERNO II.",245,245,"R6"]
["M661","LINY",125,110,"R3"]
["M681","SWEDISH",230,230,"Bello"]
["M682","SWEDISH-B",230,230,"Bello"]
["M771","RADO",115,100,"R3"]
["M991","KÖRBEMART","-","-","Választható"]
[]
["Teleajtó mintájú és üveges kivitelű ajtók, csak a fenti táblázatban szereplő minimum méretű vagy nagyobb ajtók esetében készíthetők. Üveges ajtóknál kivétel ez alól a Sapone, Sapone U, Fiume, Körbemart (R3, R6, R8, D20), Futuro minták, ezeknél az üveges minimum méret 160X160 mm, és minden oldalon 70 mm-es kerettel kell számolni."]
["A minimum magassági méreténél kisebb elemek csak fiók elő marással készíthetők.                                                                                 Sapone, Sapone U, Fiume, Körbemart(R3, R6, R8, D20), Futuro mintáknál a tele ajtó és fiók elő minta megegyezik, ezért a megadott méret, az abszolút minimumméret."]
["A minimum szélességi méretnél kisebb, bármilyen magasságú elem esetében fiók elő minta sem készíthető, csak körbemart kivitelben, a mintának megfelelő él profil marással készülhetnek."]